**Specification**

|  |  |  |
| --- | --- | --- |
| **Model** | **:** | MICHANICAL F.F.S. CUP FILLER MACHINE |
| **Description** | **:** | Fully Automatic Form, Fill & Seal Machine without Photo Electric Control  & Cup Filler |
| **Specification** | **:** | * Filling range **:** 1gm TO 15GM(DEPEND ON MATERIAL) * Speed 45 to 50 pouch per minute * Packing material **:** Heat sealable flexible laminated film * Seal type **:** three side seal * Filling system **:** cup filler * Sealing system **:** Hot bar * Electrical supply **:** 230V AC / Single Phase / 50 Hz * Power consumption 1.5 KW * Net Weight **:** 350 kg (Approx.) * Gross Weight **:** 450 kg. (Approx.) * Shipping dimension **:** 780x 650 x 1700 mm (L x W x H) |
| **Features** | **:** | * No requirement of Air compressor * Require only single phase power supply * Low power consumption * All the contacts parts made from Stainless Steel * Fitted on caster wheel |
| **Operation** | **:** | It is an Automatic Form, Fill and Seal pouch packing machine. A lay flat roll is mounted on the machine. Pouch is get formed with the help of the former. The vertical sealing takes place at top sealing rollers and horizontal sealing and cutting takes place at bottom sealing rollers. The sealing type is Hot bar sealing and it is controlled by digital temperature controller on the front panel. The filling systems is cup filler. cup of adjustment system for exact ml required. The photo control unit is used to cut the pouch at fix  place (photo dot). Batch coding (optional) is done on line on the machine |