|  |  |
| --- | --- |
| **Mr. Nitin Patel** | **Quotation No :-RW/2019-20/Q\_3929** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **3TPH Orange Oil And Juice Process Line Equipment** | | | | |
| Sr.nO | Item | Qty | Rate | Amount |
| 1 | **Elevator**   * Capacity 2-3T/H * Power 1.5kw * Dimension 3022\*600\*2600mm * Material Frame adopts 1.5-2mm 304stainless steel plate, all fruit contacting part is made of food grade 304 stainless steel * Weight About 600kg  |  | | --- | |  | | 1 | 535500 | 535500 |
| 2 | **Rolling Fruit Picking Machine**   * Capacity 2-3T/H * Power 1.5kw * Dimension 3500\*1150\*1200mm * Weight About 500kg * Material Frame adopts 1.5mm 304stainless steel plate. Food grade Nylon Belt | 1 | 1122000 | 1122000 |
| 3 | **Surfing Type Fruit Washing Machine**   * Capacity 2-3T/H * Elevating Motor Power 1.1kw * Dimension 4500\*900\*1065mm * Material Frame adopts 1.5mm 304stainless steel plate. Drive Shaft adopts 1Cr13 stainless steel * Weight About 600kg | 1 | 1130500 | 1130500 |
| 4 | **Fruit Brushing Machine**   * Capacity 2-3T/H * Power 2.2kw * Dimension 2545\*1000\*1350mm * Weight 600kg * Material Frame adopts 1.5-2mm 304stainless steel plate, all fruit contacting part is made of food grade | 1 | 1275000 | 1275000 |
| 5 | **High Lift Hoist 1**   * Capacity 2-3T/H * Power 1.5kw * Dimension 3022\*600\*2600mm * Weight 600kg * Material Frame adopts 1.5-2mm 304stainless steel plate, all fruit contacting part is made of food grade | 1 | 731000 | 731000 |
| 6 | **Orange Oil Milling Machine**   * Capacity 5T/H * Power 9kw * Dimension 5000\*2300\*2000mm * Weight About 1000kg * Material Frame adopts 1.5-2mm 304stainless steel plate ,all fruit contacting part is made of food grade | 1 | 4947000 | 4947000 |
| 7 | **Twin Screw Pressing Machine**   * Capacity 500-1000kg/h * Power 5.5kw * Dimension 3000\*950\*1300 * Weight 1200kg * Material all parts contacting fruits aremade of 304 stainless steel | 1 | 459000 | 459000 |
| 8 | **Oil-water Separator Machine**   * Capacity 2000L/H * Power 4kw * Dimension 865\*645\*1100 * Weight 550kg * Material all parts contacting fruits aremade of 304 stainless steel | 2 | 2150500 | 4301000 |
| 9 | **Screening Machine**   * Capacity 3000L/h * Power 0.75 kw * Dimension 1050\*1050\*1000 * Weight 300kg * Material all parts contacting fruits aremade of 304 stainless steel | 2 | 165750 | 331500 |
| 10 | **High Lift Elevator 2**   * Capacity 2-3 T/H * Power 1.5kw * Dimension 3022\*600\*2660mm * Weight About 600kg * Material Frame adopts 1.5-2mm 304stainless steel plate | 1 | 731000 | 731000 |
| 11 | **Orange Peeler and Juicer Machine (include a screw pump and screw conveyor)**   * Capacity 2-3T/H * Power 8 kw * Weight About 800kg * Dimension 1600\*1200\*1800 mm * Material Wall plate is made of 25mmcarbon steel outsourcing with304 stainless steel, screw pump hopper adopts 2mm 304stainless steel. * Screw Pump(receive orange pulp and convey it to next process * Screw Conveyor(To convey orange peels to other places | 1 | 2635000 | 2635000 |
| 12 | **Centrifugal Pump and slot** | 1 | 391000 | 391000 |
| 13 | **GAP Pipe**  according to its conveying length ,usually DN50)  25 m/roll | 1 | 33575 | 33575 |
| 14 | **Impeller Pump**   * Capacity 500-14000L/H * Power 1.5kw * Weight About 200kg * Material Pump chamber is 316L Stainless Steel. (import from France ) | 1 | 629000 | 629000 |
| 15 | **Centrifugal Pump**   * Capacity 1000L/H * Power 0.75kw * Weight About 200kg * Material all parts contacting fruits are made of 304 stainless steel | 3 | 104550 | 313650 |
| 16 | **Screw Pump**   * Capacity 5T/H * Power 2.2 kw * Dimension 2300\*650\*650mm * Weight About 300kg * Function Function conveying oil water mixture to the next machine | 2 | 5100 | 10200 |
| 17 | **Screw Pump**   * Capacity 3T/H * Power * 2.2 kw * Dimension 2100\*550\*550mm * Weight About 200kg * Function Conveying the material | 1 | 433500 | 433500 |
| 18 | **Juice Refine Machine (including a screw pump)**   * Capacity 2-3T/H * Dimension 2200\*900\*1330mm * Power 7.5kw * Weight About 600kg * Material Frame adopts 1.5-2mm 304stainless steel plate * **Screw Pump(**it can convey the juice into the next process | 1 | 1317500 | 1317500 |
| 19 | **Electric Carbinet** | 3 | 450500 | 1351500 |
| 20 | **Automatic 4 Head Volumetric Liquid Bottle Filling & Single Head Capping Machine**   * Direction of Movement Left to Right * Number of Filling Head 4 * Air Pressure 6 BAR * Pnuematic Items Festo * PLC Make DELTA * 12Feet CONVEYOR * FILL SIZE 200ml To 1000ml * OVERALL DIMENSION 2525 mm (L) x 1050 (W) x 1400 (H) approx, * SYRINGE SET 200ml To 1000ml * OUTPUT 800 to 1000 Ltr. per hour * Elect. Motor 1hp/ Three Phase. 50 Hz (for main machine) 0.5 hp/ Three Phase.50 Hz (For conveyor) * CONTACT PARTS S.S 316,OTHERS PARTS S.S 304 | 1 | 1025000 | 1025000 |
|  |  | |  |  |
| **Grand Total** | **2,37,03,425** |
|  | | | | |
| Raj Water Technology (Guj.) Pvt. Ltd. | | | | |

**Terms & Condition**

**1) Price**

* **The Quoted Prices Are Ex-Factory**

**2)   Payment**

* **50% Advance Along With The Purchase Order, 30% After Inspection, & 20% Before Material Dispatch.**
* **In Case Of Cancellation Of Confirmed Order Due To Any Reason, As A Part Of Penalty 25% Amount Of The Order Value Shall Have To Pay By You To Raj Water.**

**3)   Packing, Freight & Transit Insurance, & Unloading**

* **Packing Charge Will Be Extra (Depend On Packing Material)**
* **Transport To Be Arranged By The Customer OR If Arranged By Raj Water: Extra At Actual Plus GST.**
* **Transportation Insurance In The Scope Of Buyer.**
* **Unloading In The Scope Of Buyer. Buyer Has To Ready Forklift Or Crane And Unskilled Labor.**

**4)  Delivery**

* **Schedule For Dispatch Will Be Notified.**
  + **Delivery Dates Are Approximate Only, And Assume Timely Receipt Of All Information, Test Materials & Payment.**

**5)   Warranty**

* **We Shall Provide 1 Year Warranty For The Following:**
* **Manufacturing Defects, Raw Water Pump, High Pressure Pump, Treated Water Transfer Pump.**
* **Due To Fluctuation In Power Supply, Attempted Repaired By Person Other Than Our Technical Representative, Improper Handling Or Negligence By End Users, Poor Maintenance, Improper Use Of Equipment, That All Type Of Damage Not Covered In Warranty Create Area.**
* **During The Warranty Period, We Shall Provide Supervisory Services Of Our Technical Representative As And When Required.**

**6)    Accommodation**

* **Technician Charge Will Be Extra 1000/- Rs. Per Day.**
* **Travelling, Lodging And Boarding, Local Conveyance And Any Other Miscellaneous Expense Of Our Technical Representative Will Have To Be Borne By Client.**

**7)   Validity**

* **Our Offer Is Valid For Your Acceptance For A Period Of 6 Months From The Date; Thereafter It Will Be Subject To Confirmation By Us.**

**8)    Image:-Images Are For Representation Purpose Only.**

**9)  Jurisdiction:-All Terms Subject To Rajkot ,Gujarat Jurisdiction**